A logo for a machine tool

Description automatically generated Stelly Machine Tool, Inc

275 Happy Street

Church Point La, 70525

Phone 337.298.7104

Email: [cstellysr@gmail.com](mailto:cstellysr@gmail.com)

Web: www.stellymachinetools.com

We are pleased to quote the following for your consideration

**OKUMA Multus B750W 4000**

THE YEAR 2015

MFG OKUMA

MODEL Multus B750W 4000

**SPECIFICATIONS:**

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
| **Item** | **Description** | **Quantity** | **Comment** |
| B-5R8-04000-19 | MULTUS B750W X 4000 | 1.00 |  |
| C-5R8-1295-9 | ATC 160 CAPTO-C8 | 1.00 |  |
| C-5R8-2017-9 | CONVEYOR, SIDE BCD4000 | 1.00 |  |
| C-5R8-2108-9 | AUTO DOOR BOTH W/ DUAL CYCLE | 1.00 |  |
| C-5R8-2803-9 | TOUCHSETTER A | 1.00 |  |
| C-5R8-6067-9 | HYDRAULIC OIL TEMP.REG AKZ148 | 1.00 |  |
| C-5R8-6306-9 | PREP FOR MIST COLLECTOR | 1.00 |  |
| C-5R8-6611-9 | LONG BORING BAR SPEC | 1.00 |  |
| C-5R8-6612-9 | LONG BORING BAR (BAR ONLY) | 1.00 | 120mm x 1000mm |
| C-5R8-8163-9 | LATHE TOOL INDEX FUNCTION | 1.00 |  |
| C-5R8-8249-9 | C-AXIS SYNCHRONIZE FUNCTION | 1.00 |  |
| C-5R8-8251-9 | C-AXIS AUTO ZERO OFFSET FUNCT | 2.00 | Main and Sub-Spindle |
| C-5R8-8253-9 | Z-AXIS AUTO ZERO OFFSET FUNCT | 2.00 | Main and Sub-Spindle |
| C-5R8-8254-9 | OFF-CENTER TURNING FUNCTION | 1.00 |  |
| C-5R8-82A1-9 | TMAC8 ADAPTIVE CONT/MON SYSTEM | 1.00 |  |
| C-5R8-8304-9 | SPARE M-CODES, 8 SETS | 1.00 |  |
| C-5R8-8338-9 | FEED HOLD DURING THREADING | 1.00 |  |
| C-5R8-8339-9 | THREAD START POINT OFFSET | 1.00 |  |
| C-5R8-8375-9 | DNC T3 | 1.00 |  |
| C-5R8-8383-9 | VAR SPIN SPD THREAD-MAIN OR2ND | 1.00 |  |
| C-5R8-8390-9 | NEGATIVE TOOL RADIUS COMP | 1.00 |  |
| C-917-9011-9 | UL PREP SPEC | 1.00 |  |
| C-5R8-8274-9 | ROBOT/LOADER I/F ANYBUS-X EIP | 1.00 |  |
| C-SFT-8252-9 | Y-AXIS GAUGING | 1.00 |  |
| C-5R8-2773-9 | AUTO GAUGING REN RMP60 CAPTOC8 | 1.00 |  |
| C-5R8-3517-9 | PREP FOR SLU-Z 5.1 STEADYREST SMW | 1.00 |  |
| C-5R8-8224-9 | EXT PROG SEL C2 BCD ABX EIP | 1.00 |  |
| C-5R8-LBBHOLDER1 | LBB TOOL HOLDER MAIN/C-CLOCK | 1.00 |  |
| C-5R8-LBBHOLDER2 | LBB TOOL HOLDER MAIN/C-CLOCK | 1.00 |  |
| C-U5600-05R8-015 | LBB BASE FLANGE (MANUAL TYPE) | 3.00 |  |

**Equipped With**:

P300

2-Losmas Mist Collectors

Caron Engineering RFID